Router>

Router>exit

Router>

Router>

Router>ena

Password:123

Router#conf t

int g0/0/0

ip address 192.168.1.1 255.255.255.0

no shutdown

Enter configuration commands, one per line. End with CNTL/Z.

# Reset

Shutdown after ctrl+c after write: confreg after yes no, no, ye ,no,no,no reset reload

RESETTING ROUTER

CTRL+C> when it starting;

Type confreg;

Press yes>no>no>yes>no>no>no

>reset

Then wait the resetting process.

Connect pc to router >open putty>

Click start>computer management>device manager>choose port>

Basic configurations

RP-Musanze>en

Password:

RP-Musanze#conf t

Enter configuration commands, one per line. End with CNTL/Z.

RP-Musanze(config)#int g0/0/0

RP-Musanze(config-if)#ip address 192.168.1.1 255.255.255.0

RP-Musanze(config-if)#no shut

RP-Musanze(config-if)#no shutdown

RP-Musanze(config-if)#exit

RP-Musanze(config)#lin

RP-Musanze(config)#line v

RP-Musanze(config)#line vty 0 15

RP-Musanze(config-line)#pass

RP-Musanze(config-line)#password 123

RP-Musanze(config-line)#ena

RP-Musanze(config-line)#lo

RP-Musanze(config-line)#logi

RP-Musanze(config-line)#login

RP-Musanze(config-line)#exit

RP-Musanze(config)#ena

RP-Musanze(config)#enable pass

RP-Musanze(config)#enable password 123

RP-Musanze(config)#do wr

RP-Musanze(config)#dos show run